,Part Number##other##,Model Series##other##,Description##other##,Front Door Solid##Other##,Front Door Plexi##Other##,Front Door Vented 25%##Other##,Front Door Vented 64%##Other##,Front Door Plexi Vented##Other##,Rear Doors Partially Vented##Other##,Rear Door Standard##other##,Weight Product##Force##Pounds,Overall Height##Length##Inches,Useable Height##Length##inches,Overall Depth##Length##Inches,Useable Depth##Length##Inches,Bottom Opening Depth##Length##Inches,Safety Rating##other##,Sustainability Rating##other##,MasterFormat##other##,OmniClass##other##,IQ Category##other##,URL##other##,Product URL##other##,Seismic Rating##other##,Accessory Part 1 Number##Other##,Accessory Part 1 Long Description##Other##,Accessory Part 1 Short Description##Other##,Accessory Part 1 UPC Product Code##Other##,Accessory Part 1 Weight##Force##Pounds,Accessory Part 1 Terminated##Other##,Accessory Part 1 Circuit##Other##,Accessory Part 1 Outlets##Other##,Accessory Part 1 Overall##Other##,Accessory Part 1 Qty##Other##,Accessory Part 2 Number##other##,Accessory Part 2 Long Description##Other##,Accessory Part 2 Short Description##Other##,Accessory Part 2 UPC Product Code##Other##,Accessory Part 2 Weight##Force##Pounds,Accessory Part 3 Number##Other##,Accessory Part 3 Long Description##Other##,Accessory Part 3 Short Description##Other##,Accessory Part 3 UPC Product Code##Other##,Accessory Part 3 Weight##Force##Pounds,Accessory Part 4 Number##Other##,Accessory Part 4 Long Description##Other##,Accessory Part 4 Short Description##Other##,Accessory Part 4 UPC Product Code##Other##,Accessory Part 4 Weight##Force##Pounds,Accessory Part 5 Number##Other##,Accessory Part 5 Long Description##Other##,Accessory Part 5 Short Description##Other##,Accessory Part 5 UPC Product Code##Other##,Accessory Part 5 Weight##Force##Pounds,Accessory Part 6 Number##Other##,Accessory Part 6 Long Description##Other##,Accessory Part 6 Short Description##Other##,Accessory Part 6 UPC Product Code##Other##,Accessory Part 6 Weight##Force##Pounds,Accessory Part 7 Number##Other##,Accessory Part 7 Long Description##Other##,Accessory Part 7 Short Description##Other##,Accessory Part 7 UPC Product Code##Other##,Accessory Part 7 Weight##Force##Pounds,Accessory Part 8 Number##Other##,Accessory Part 8 Long Description##Other##,Accessory Part 8 Short Description##Other##,Accessory Part 8 UPC Product Code##Other##,Accessory Part 8 Weight##Force##Pounds,Accessory Part 9 Number##Other##,Accessory Part 9 Long Description##Other##,Accessory Part 9 Short Description##Other##,Accessory Part 9 UPC Product Code##Other##,Accessory Part 9 Weight##Force##Pounds,Accessory Part 10 Number##Other##,Accessory Part 10 Long Description##Other##,Accessory Part 10 Short Description##Other##,Accessory Part 10 UPC Product Code##Other##,Accessory Part 10 Weight##Force##Pounds,Accessory Part 11 Number##Other##,Accessory Part 11 Long Description##Other##,Accessory Part 11 Short Description##Other##,Accessory Part 11 UPC Product Code##Other##,Accessory Part 11 Weight##Force##Pounds,Accessory Part 12 Number##Other##,Accessory Part 12 Long Description##Other##,Accessory Part 12 Short Description##Other##,Accessory Part 12 UPC Product Code##Other##,Accessory Part 12 Weight##Force##Pounds,Accessory Part 13 Number##Other##,Accessory Part 13 Long Description##Other##,Accessory Part 13 Short Description##Other##,Accessory Part 13 UPC Product Code##Other##,Accessory Part 13 Weight##Force##Pounds,Accessory Part 14 Number##Other##,Accessory Part 14 Long Description##Other##,Accessory Part 14 Short Description##Other##,Accessory Part 14 UPC Product Code##Other##,Accessory Part 14 Weight##Force##Pounds,Top Option Available##Other##,Front Door_Solid##other##,Front Door_Plexiglas##other##,Rear Door_Split##other##,Rear Door_Single##other##
ERK-1820 (No Front - Standard Rear),ERK-1820,ERK SERIES,"19"" STAND ALONE ENCLOSURE 18 SPACE 31.5"" RACKING HEIGHT",,,,,,,Included,94.00,35.63,31.63,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR18,"11 GAUGE, 10-32 THREADED 18 SPACE ADDITIONAL RAIL KIT, MOUNTING HARDWARE INCLUDED",18SP ERK REAR RAIL OPTION,,6.70,ERK-RR18,18 SPACE (31.50) ERK REAR RAIL KIT,18SP ERK REAR RAIL ,,6.70,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,0,0,1
ERK-1820 (Solid Front - Standard Rear),ERK-1820,ERK SERIES,"19"" STAND ALONE ENCLOSURE 18 SPACE 31.5"" RACKING HEIGHT",FD-18,,,,,,Included,94.00,35.63,31.63,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR18,"11 GAUGE, 10-32 THREADED 18 SPACE ADDITIONAL RAIL KIT, MOUNTING HARDWARE INCLUDED",18SP ERK REAR RAIL OPTION,,6.70,ERK-RR18,18 SPACE (31.50) ERK REAR RAIL KIT,18SP ERK REAR RAIL ,,6.70,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-1820 (Plexiglas Front - Standard Rear),ERK-1820,ERK SERIES,"19"" STAND ALONE ENCLOSURE 18 SPACE 31.5"" RACKING HEIGHT",,PFD-18,,,,,Included,94.00,35.63,31.63,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR18,"11 GAUGE, 10-32 THREADED 18 SPACE ADDITIONAL RAIL KIT, MOUNTING HARDWARE INCLUDED",18SP ERK REAR RAIL OPTION,,6.70,ERK-RR18,18 SPACE (31.50) ERK REAR RAIL KIT,18SP ERK REAR RAIL ,,6.70,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,1,0,1
ERK-1820 (Vented Front 25%  - Standard Rear),ERK-1820,ERK SERIES,"19"" STAND ALONE ENCLOSURE 18 SPACE 31.5"" RACKING HEIGHT",,,VFD-18,,,,Included,94.00,35.63,31.63,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR18,"11 GAUGE, 10-32 THREADED 18 SPACE ADDITIONAL RAIL KIT, MOUNTING HARDWARE INCLUDED",18SP ERK REAR RAIL OPTION,,6.70,ERK-RR18,18 SPACE (31.50) ERK REAR RAIL KIT,18SP ERK REAR RAIL ,,6.70,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-1820 (Vented Front 64%  - Standard Rear),ERK-1820,ERK SERIES,"19"" STAND ALONE ENCLOSURE 18 SPACE 31.5"" RACKING HEIGHT",,,,LVFD-18,,,Included,94.00,35.63,31.63,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR18,"11 GAUGE, 10-32 THREADED 18 SPACE ADDITIONAL RAIL KIT, MOUNTING HARDWARE INCLUDED",18SP ERK REAR RAIL OPTION,,6.70,ERK-RR18,18 SPACE (31.50) ERK REAR RAIL KIT,18SP ERK REAR RAIL ,,6.70,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-1825 (No Front - Standard Rear),ERK-1825,ERK SERIES,"19"" STAND ALONE ENCLOSURE 18 SPACE 31.5"" RACKING HEIGHT",,,,,,,Included,104.00,35.63,31.63,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR18,18 SPACE (31.50) ERK REAR RAIL KIT,18SP ERK REAR RAIL ,,6.70,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,0,0,1
ERK-1825 (Solid Front - Standard Rear),ERK-1825,ERK SERIES,"19"" STAND ALONE ENCLOSURE 18 SPACE 31.5"" RACKING HEIGHT",FD-18,,,,,,Included,104.00,35.63,31.63,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR18,18 SPACE (31.50) ERK REAR RAIL KIT,18SP ERK REAR RAIL ,,6.70,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-1825 (Plexiglas Front - Standard Rear),ERK-1825,ERK SERIES,"19"" STAND ALONE ENCLOSURE 18 SPACE 31.5"" RACKING HEIGHT",,PFD-18,,,,,Included,104.00,35.63,31.63,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR18,18 SPACE (31.50) ERK REAR RAIL KIT,18SP ERK REAR RAIL ,,6.70,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,1,0,1
ERK-1825 (Vented Front 25% - Standard Rear),ERK-1825,ERK SERIES,"19"" STAND ALONE ENCLOSURE 18 SPACE 31.5"" RACKING HEIGHT",,,VFD-18,,,,Included,104.00,35.63,31.63,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR18,18 SPACE (31.50) ERK REAR RAIL KIT,18SP ERK REAR RAIL ,,6.70,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-1825 (Vented Front 64% - Standard Rear),ERK-1825,ERK SERIES,"19"" STAND ALONE ENCLOSURE 18 SPACE 31.5"" RACKING HEIGHT",,,,LVFD-18,,,Included,104.00,35.63,31.63,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR18,18 SPACE (31.50) ERK REAR RAIL KIT,18SP ERK REAR RAIL ,,6.70,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2120 (No Front - Standard Rear),ERK-2120,ERK SERIES,"19"" STAND ALONE ENCLOSURE 21 SPACE 36.75"" RACKING HEIGHT",,,,,,,Included,100.00,40.88,38.88,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR21,"11 GAUGE, 10-32 THREADED, 21 SPACE ADDITIONAL RAIL KIT, MOUNTING HARDWARE INCLUDED",21SP ERK REAR RAIL OPTION,,7.90,ERK-RR21,21 SPACE (36.75) ERK REAR RAIL KIT,21SP ERK REAR RAIL ,,7.90,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,0,0,1
ERK-2120 (Solid Front - Standard Rear),ERK-2120,ERK SERIES,"19"" STAND ALONE ENCLOSURE 21 SPACE 36.75"" RACKING HEIGHT",FD-21,,,,,,Included,100.00,40.88,38.88,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR21,"11 GAUGE, 10-32 THREADED, 21 SPACE ADDITIONAL RAIL KIT, MOUNTING HARDWARE INCLUDED",21SP ERK REAR RAIL OPTION,,7.90,ERK-RR21,21 SPACE (36.75) ERK REAR RAIL KIT,21SP ERK REAR RAIL ,,7.90,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2120 (Plexiglas Front - Standard Rear),ERK-2120,ERK SERIES,"19"" STAND ALONE ENCLOSURE 21 SPACE 36.75"" RACKING HEIGHT",,PFD-21,,,,,Included,100.00,40.88,38.88,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR21,"11 GAUGE, 10-32 THREADED, 21 SPACE ADDITIONAL RAIL KIT, MOUNTING HARDWARE INCLUDED",21SP ERK REAR RAIL OPTION,,7.90,ERK-RR21,21 SPACE (36.75) ERK REAR RAIL KIT,21SP ERK REAR RAIL ,,7.90,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,1,0,1
ERK-2120 (Vented Front 25% - Standard Rear),ERK-2120,ERK SERIES,"19"" STAND ALONE ENCLOSURE 21 SPACE 36.75"" RACKING HEIGHT",,,VFD-21,,,,Included,100.00,40.88,38.88,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR21,"11 GAUGE, 10-32 THREADED, 21 SPACE ADDITIONAL RAIL KIT, MOUNTING HARDWARE INCLUDED",21SP ERK REAR RAIL OPTION,,7.90,ERK-RR21,21 SPACE (36.75) ERK REAR RAIL KIT,21SP ERK REAR RAIL ,,7.90,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2120 (Vented Front 64% - Standard Rear),ERK-2120,ERK SERIES,"19"" STAND ALONE ENCLOSURE 21 SPACE 36.75"" RACKING HEIGHT",,,,LVFD-21,,,Included,100.00,40.88,38.88,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR21,"11 GAUGE, 10-32 THREADED, 21 SPACE ADDITIONAL RAIL KIT, MOUNTING HARDWARE INCLUDED",21SP ERK REAR RAIL OPTION,,7.90,ERK-RR21,21 SPACE (36.75) ERK REAR RAIL KIT,21SP ERK REAR RAIL ,,7.90,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2125 (No Front  - Standard Rear),ERK-2125,ERK SERIES,"19"" STAND ALONE ENCLOSURE 21 SPACE 36.75"" RACKING HEIGHT",,,,,,,Included,118.00,40.88,36.88,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR21,21 SPACE (36.75) ERK REAR RAIL KIT,21SP ERK REAR RAIL ,,7.90,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,0,0,1
ERK-2125 (Solid Front - Standard Rear),ERK-2125,ERK SERIES,"19"" STAND ALONE ENCLOSURE 21 SPACE 36.75"" RACKING HEIGHT",FD-21,,,,,,Included,118.00,40.88,36.88,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR21,21 SPACE (36.75) ERK REAR RAIL KIT,21SP ERK REAR RAIL ,,7.90,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2125 (Plexiglas Front - Standard Rear,ERK-2125,ERK SERIES,"19"" STAND ALONE ENCLOSURE 21 SPACE 36.75"" RACKING HEIGHT",,PFD-21,,,,,Included,118.00,40.88,36.88,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR21,21 SPACE (36.75) ERK REAR RAIL KIT,21SP ERK REAR RAIL ,,7.90,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,1,0,1
ERK-2125 (Vented Front 25% - Standard Rear),ERK-2125,ERK SERIES,"19"" STAND ALONE ENCLOSURE 21 SPACE 36.75"" RACKING HEIGHT",,,VFD-21,,,,Included,118.00,40.88,36.88,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR21,21 SPACE (36.75) ERK REAR RAIL KIT,21SP ERK REAR RAIL ,,7.90,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2125 (Vented Front 64% - Standard Rear),ERK-2125,ERK SERIES,"19"" STAND ALONE ENCLOSURE 21 SPACE 36.75"" RACKING HEIGHT",,,,LVFD-21,,,Included,118.00,40.88,36.88,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR21,21 SPACE (36.75) ERK REAR RAIL KIT,21SP ERK REAR RAIL ,,7.90,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2720 (No Front - Standard Rear),ERK-2720,ERK SERIES,"19"" STAND ALONE ENCLOSURE 27 SPACE 47.5"" RACKING HEIGHT",,,,,,,Included,116.00,51.38,47.38,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR27,"11 GAUGE, 10-32 THREADED, 27 SPACE ADDITIONAL RAIL KIT,  MOUNTING HARDWARE INCLUDED",27SP ERK REAR RAIL OPTION,,10.10,ERK-RR27,27 SPACE (47.25) ERK REAR RAIL KIT,27SP ERK REAR RAIL ,,10.10,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,0,0,1
ERK-2720 (Solid Front - Standard Rear),ERK-2720,ERK SERIES,"19"" STAND ALONE ENCLOSURE 27 SPACE 47.5"" RACKING HEIGHT",FD-27,,,,,,Included,116.00,51.38,47.38,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR27,"11 GAUGE, 10-32 THREADED, 27 SPACE ADDITIONAL RAIL KIT,  MOUNTING HARDWARE INCLUDED",27SP ERK REAR RAIL OPTION,,10.10,ERK-RR27,27 SPACE (47.25) ERK REAR RAIL KIT,27SP ERK REAR RAIL ,,10.10,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2720 (Plexiglas Front - Standard Rear),ERK-2720,ERK SERIES,"19"" STAND ALONE ENCLOSURE 27 SPACE 47.5"" RACKING HEIGHT",,PFD-27,,,,,Included,116.00,51.38,47.38,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR27,"11 GAUGE, 10-32 THREADED, 27 SPACE ADDITIONAL RAIL KIT,  MOUNTING HARDWARE INCLUDED",27SP ERK REAR RAIL OPTION,,10.10,ERK-RR27,27 SPACE (47.25) ERK REAR RAIL KIT,27SP ERK REAR RAIL ,,10.10,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,1,0,1
ERK-2720 (Vented Front  25% - Standard Rear),ERK-2720,ERK SERIES,"19"" STAND ALONE ENCLOSURE 27 SPACE 47.5"" RACKING HEIGHT",,,VFD-27,,,,Included,116.00,51.38,47.38,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR27,"11 GAUGE, 10-32 THREADED, 27 SPACE ADDITIONAL RAIL KIT,  MOUNTING HARDWARE INCLUDED",27SP ERK REAR RAIL OPTION,,10.10,ERK-RR27,27 SPACE (47.25) ERK REAR RAIL KIT,27SP ERK REAR RAIL ,,10.10,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2720 (Vented Front 64% - Standard Rear),ERK-2720,ERK SERIES,"19"" STAND ALONE ENCLOSURE 27 SPACE 47.5"" RACKING HEIGHT",,,,LVFD-27,,,Included,116.00,51.38,47.38,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR27,"11 GAUGE, 10-32 THREADED, 27 SPACE ADDITIONAL RAIL KIT,  MOUNTING HARDWARE INCLUDED",27SP ERK REAR RAIL OPTION,,10.10,ERK-RR27,27 SPACE (47.25) ERK REAR RAIL KIT,27SP ERK REAR RAIL ,,10.10,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2725 (No Front - Standard Rear),ERK-2725,ERK SERIES,"19"" STAND ALONE ENCLOSURE 27 SPACE 47.5"" RACKING HEIGHT",,,,,,,Included,132.00,51.38,47.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR27,27 SPACE (47.25) ERK REAR RAIL KIT,27SP ERK REAR RAIL ,,10.10,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,1,0,1
ERK-2725 (Solid Front - Standard Rear),ERK-2725,ERK SERIES,"19"" STAND ALONE ENCLOSURE 27 SPACE 47.5"" RACKING HEIGHT",FD-27,,,,,,Included,132.00,51.38,47.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR27,27 SPACE (47.25) ERK REAR RAIL KIT,27SP ERK REAR RAIL ,,10.10,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2725 (Plexiglas Front - Standard Rear),ERK-2725,ERK SERIES,"19"" STAND ALONE ENCLOSURE 27 SPACE 47.5"" RACKING HEIGHT",,PFD-27,,,,,Included,132.00,51.38,47.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR27,27 SPACE (47.25) ERK REAR RAIL KIT,27SP ERK REAR RAIL ,,10.10,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,1,0,1
ERK-2725 (Vented Front 25% - Standard Rear),ERK-2725,ERK SERIES,"19"" STAND ALONE ENCLOSURE 27 SPACE 47.5"" RACKING HEIGHT",,,VFD-27,,,,Included,132.00,51.38,47.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR27,27 SPACE (47.25) ERK REAR RAIL KIT,27SP ERK REAR RAIL ,,10.10,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2725 (Vented Front 64% - Standard Rear),ERK-2725,ERK SERIES,"19"" STAND ALONE ENCLOSURE 27 SPACE 47.5"" RACKING HEIGHT",,,,LVFD-27,,,Included,132.00,51.38,47.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR27,27 SPACE (47.25) ERK REAR RAIL KIT,27SP ERK REAR RAIL ,,10.10,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-3520 (No Front- Standard Rear),ERK-3520,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT",,,,,,,Included,136.00,65.38,61.38,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR35,"11 GAUGE, 10-32 THREADED, 35 SPACE ADDITIONAL RAIL KIT MOUNTING HARDWARE INCLUDED",35SP ERK REAR RAIL OPTION,,12.20,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, FITS ANY 35"" SPACE RACKS, BLACK FINISH",4.5 (3) FAN TOP,,0.00,NONE,NONE,NONE,,0.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,0,0,1
ERK-3520 (Solid Front - Standard Rear),ERK-3520,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT",FD-35,,,,,,Included,136.00,65.38,61.38,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR35,"11 GAUGE, 10-32 THREADED, 35 SPACE ADDITIONAL RAIL KIT MOUNTING HARDWARE INCLUDED",35SP ERK REAR RAIL OPTION,,12.20,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, FITS ANY 35"" SPACE RACKS, BLACK FINISH",4.5 (3) FAN TOP,,0.00,NONE,NONE,NONE,,0.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-3520 (Plexiglas Front  - Standard Rear),ERK-3520,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT",,PFD-35,,,,,Included,136.00,65.38,61.38,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR35,"11 GAUGE, 10-32 THREADED, 35 SPACE ADDITIONAL RAIL KIT MOUNTING HARDWARE INCLUDED",35SP ERK REAR RAIL OPTION,,12.20,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, FITS ANY 35"" SPACE RACKS, BLACK FINISH",4.5 (3) FAN TOP,,0.00,NONE,NONE,NONE,,0.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-3520 (Vented Front 25% - Standard Rear),ERK-3520,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT",,,VFD-35,,,,Included,136.00,65.38,61.38,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR35,"11 GAUGE, 10-32 THREADED, 35 SPACE ADDITIONAL RAIL KIT MOUNTING HARDWARE INCLUDED",35SP ERK REAR RAIL OPTION,,12.20,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, FITS ANY 35"" SPACE RACKS, BLACK FINISH",4.5 (3) FAN TOP,,0.00,NONE,NONE,NONE,,0.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-3520 (Vented Front 64% - Standard Rear),ERK-3520,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT",,,,LVFD-35,,,Included,136.00,65.38,61.38,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR35,"11 GAUGE, 10-32 THREADED, 35 SPACE ADDITIONAL RAIL KIT MOUNTING HARDWARE INCLUDED",35SP ERK REAR RAIL OPTION,,12.20,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, FITS ANY 35"" SPACE RACKS, BLACK FINISH",4.5 (3) FAN TOP,,0.00,NONE,NONE,NONE,,0.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-3525 (No Front - Standard Rear),ERK-3525,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT",,,,,,,Included,156.00,65.38,61.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,0,0,1
ERK-3525 (Solid Front - Standard Rear),ERK-3525,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT",FD-35,,,,,,Included,156.00,65.38,61.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-3525 (Plexiglas Front  - Standard Rear),ERK-3525,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT",,PFD-35,,,,,Included,156.00,65.38,61.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-3525 (Vented Front 25% - Standard Rear),ERK-3525,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT",,,VFD-35,,,,Included,156.00,65.38,61.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-3525 (Vented Front 64% - Standard Rear),ERK-3525,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT",,,,LVFD-35,,,Included,156.00,65.38,61.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-3525-AV (No Front - Standard Rear),ERK-3525-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT WITH TWO 10 OUTLET THIN POWER STRIPS",,,,,,,Included,210.00,63.39,61.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-1020-NS,10 OUTLET SINGLE 20 AMP CIRCUIT THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT 'G' POWER,"PD THIN, 1-20A, 10 OUT, CORD",,4.40,5-20P,20 AMP,"10, 5-20R",37.75,1,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-37-OP,"64.75"" HEIGHT 3 1/4"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 64-3/4H X 3-1/4W SLOT LCER,,23.10,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,LACE-35-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-3525-AV 37 RACK SPACES",6PC 64-3/4H X 3-1/4W SLOT LCER,,23.10,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,0,0,1
ERK-3525-AV (Solid Front - Standard Rear),ERK-3525-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT WITH TWO 10 OUTLET THIN POWER STRIPS",INCLUDED,,,,,,Included,210.00,63.39,61.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-1020-NS,10 OUTLET SINGLE 20 AMP CIRCUIT THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT 'G' POWER,"PD THIN, 1-20A, 10 OUT, CORD",,4.40,5-20P,20 AMP,"10, 5-20R",37.75,1,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-37-OP,"64.75"" HEIGHT 3 1/4"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 64-3/4H X 3-1/4W SLOT LCER,,23.10,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,LACE-35-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-3525-AV 37 RACK SPACES",6PC 64-3/4H X 3-1/4W SLOT LCER,,23.10,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-3525-AV (Plexiglas Front - Standard Rear),ERK-3525-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT WITH TWO 10 OUTLET THIN POWER STRIPS",,PFD-35,,,,,Included,210.00,63.39,61.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-1020-NS,10 OUTLET SINGLE 20 AMP CIRCUIT THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT 'G' POWER,"PD THIN, 1-20A, 10 OUT, CORD",,4.40,5-20P,20 AMP,"10, 5-20R",37.75,1,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-37-OP,"64.75"" HEIGHT 3 1/4"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 64-3/4H X 3-1/4W SLOT LCER,,23.10,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,LACE-35-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-3525-AV 37 RACK SPACES",6PC 64-3/4H X 3-1/4W SLOT LCER,,23.10,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-3525-AV (Vented Front 25% - Standard Rear),ERK-3525-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT WITH TWO 10 OUTLET THIN POWER STRIPS",,,VFD-35,,,,Included,210.00,63.39,61.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-1020-NS,10 OUTLET SINGLE 20 AMP CIRCUIT THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT 'G' POWER,"PD THIN, 1-20A, 10 OUT, CORD",,4.40,5-20P,20 AMP,"10, 5-20R",37.75,1,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-37-OP,"64.75"" HEIGHT 3 1/4"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 64-3/4H X 3-1/4W SLOT LCER,,23.10,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,LACE-35-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-3525-AV 37 RACK SPACES",6PC 64-3/4H X 3-1/4W SLOT LCER,,23.10,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-3525-AV (Vented Front 64% - Standard Rear),ERK-3525-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT WITH TWO 10 OUTLET THIN POWER STRIPS",,,,LVFD-35,,,Included,210.00,63.39,61.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-1020-NS,10 OUTLET SINGLE 20 AMP CIRCUIT THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT 'G' POWER,"PD THIN, 1-20A, 10 OUT, CORD",,4.40,5-20P,20 AMP,"10, 5-20R",37.75,1,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-37-OP,"64.75"" HEIGHT 3 1/4"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 64-3/4H X 3-1/4W SLOT LCER,,23.10,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,LACE-35-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-3525-AV 37 RACK SPACES",6PC 64-3/4H X 3-1/4W SLOT LCER,,23.10,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4020 (No Front - Standard Rear),ERK-4020,ERK SERIES,"19"" STAND ALONE ENCLOSURE 40 SPACE 70"" RACKING HEIGHT",,,,,,,Included,150.00,74.13,70.13,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR40,"11 GAUGE, 10-32 THREADED, 40 SPACE ADDITIONAL RAIL KIT MOUNTING HARDWARE INCLUDED",40SP ERK REAR RAIL OPTION,,14.30,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL ,,14.30,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, FITS 35+ SPACE RACKS BLACK FINISH",4.5 (3) FAN TOP,,0.00,NONE,NONE,NONE,,0.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,0,0,1
ERK-4020 (Solid Front - Standard Rear),ERK-4020,ERK SERIES,"19"" STAND ALONE ENCLOSURE 40 SPACE 70"" RACKING HEIGHT",FD-40,,,,,,Included,150.00,74.13,70.13,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR40,"11 GAUGE, 10-32 THREADED, 40 SPACE ADDITIONAL RAIL KIT MOUNTING HARDWARE INCLUDED",40SP ERK REAR RAIL OPTION,,14.30,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL ,,14.30,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, FITS 35+ SPACE RACKS BLACK FINISH",4.5 (3) FAN TOP,,0.00,NONE,NONE,NONE,,0.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4020 (Plexiglas Front - Standard Rear),ERK-4020,ERK SERIES,"19"" STAND ALONE ENCLOSURE 40 SPACE 70"" RACKING HEIGHT",,PFD-40,,,,,Included,150.00,74.13,70.13,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR40,"11 GAUGE, 10-32 THREADED, 40 SPACE ADDITIONAL RAIL KIT MOUNTING HARDWARE INCLUDED",40SP ERK REAR RAIL OPTION,,14.30,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL ,,14.30,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, FITS 35+ SPACE RACKS BLACK FINISH",4.5 (3) FAN TOP,,0.00,NONE,NONE,NONE,,0.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-4020 (Vented Front 25% - Standard Rear),ERK-4020,ERK SERIES,"19"" STAND ALONE ENCLOSURE 40 SPACE 70"" RACKING HEIGHT",,,VFD-40,,,,Included,150.00,74.13,70.13,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR40,"11 GAUGE, 10-32 THREADED, 40 SPACE ADDITIONAL RAIL KIT MOUNTING HARDWARE INCLUDED",40SP ERK REAR RAIL OPTION,,14.30,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL ,,14.30,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, FITS 35+ SPACE RACKS BLACK FINISH",4.5 (3) FAN TOP,,0.00,NONE,NONE,NONE,,0.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4020 (Vented Front 64% - Standard Rear),ERK-4020,ERK SERIES,"19"" STAND ALONE ENCLOSURE 40 SPACE 70"" RACKING HEIGHT",,,,LVFD-40,,,Included,150.00,74.13,70.13,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR40,"11 GAUGE, 10-32 THREADED, 40 SPACE ADDITIONAL RAIL KIT MOUNTING HARDWARE INCLUDED",40SP ERK REAR RAIL OPTION,,14.30,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL ,,14.30,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, FITS 35+ SPACE RACKS BLACK FINISH",4.5 (3) FAN TOP,,0.00,NONE,NONE,NONE,,0.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4025 (No Front - Standard Rear),ERK-4025,ERK SERIES,"19"" STAND ALONE ENCLOSURE 40 SPACE WITH TWO 10 OUTLET THIN POWER STRIPS",,,,,,,Included,190.00,74.13,70.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL ,,14.30,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,0,0,1
ERK-4025 (Solid Front - Standard Rear),ERK-4025,ERK SERIES,"19"" STAND ALONE ENCLOSURE 40 SPACE WITH TWO 10 OUTLET THIN POWER STRIPS",FD-40,,,,,,Included,190.00,74.13,70.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL ,,14.30,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4025 (Plexiglas Front - Standard Rear),ERK-4025,ERK SERIES,"19"" STAND ALONE ENCLOSURE 40 SPACE WITH TWO 10 OUTLET THIN POWER STRIPS",,PFD-40,,,,,Included,190.00,74.13,70.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL ,,14.30,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-4025 (Vented Front 25% - Standard Rear),ERK-4025,ERK SERIES,"19"" STAND ALONE ENCLOSURE 40 SPACE WITH TWO 10 OUTLET THIN POWER STRIPS",,,VFD-40,,,,Included,190.00,74.13,70.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL ,,14.30,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4025 (Vented Front 64% - Standard Rear),ERK-4025,ERK SERIES,"19"" STAND ALONE ENCLOSURE 40 SPACE WITH TWO 10 OUTLET THIN POWER STRIPS",,,,LVFD-40,,,Included,190.00,74.13,70.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL ,,14.30,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4025-AV (No Front - Standard Rear),ERK-4025-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE, 40 SPACE 70"" RACKING HEIGHT WITH TWO 20 OUTLET THIN POWER STRIPS",,,,,,,Included,170.00,74.13,70.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-1020-NS,10 OUTLET SINGLE 20 AMP CIRCUIT THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT 'G' POWER,"PD THIN, ONE 20A, 10 OUT CORD",,4.40,5-20P,20 AMP,"10, 5-20R",37.75,1,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-40-OP,"70"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 70H X 3-1/4W SLOT LACER,,24.80,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL,,14.30,LACE-40-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4025-AV 40 RACK SPACES",6PC 70H X 3-1/4W SLOT LACER,,24.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,0,0,1
ERK-4025-AV (Solid Front - Standard Rear),ERK-4025-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE, 40 SPACE 70"" RACKING HEIGHT WITH TWO 20 OUTLET THIN POWER STRIPS",FD-40,,,,,,Included,170.00,74.13,70.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-1020-NS,10 OUTLET SINGLE 20 AMP CIRCUIT THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT 'G' POWER,"PD THIN, ONE 20A, 10 OUT CORD",,4.40,5-20P,20 AMP,"10, 5-20R",37.75,1,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-40-OP,"70"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 70H X 3-1/4W SLOT LACER,,24.80,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL,,14.30,LACE-40-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4025-AV 40 RACK SPACES",6PC 70H X 3-1/4W SLOT LACER,,24.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4025-AV (Plexiglas Front - Standard Rear),ERK-4025-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE, 40 SPACE 70"" RACKING HEIGHT WITH TWO 20 OUTLET THIN POWER STRIPS",,PFD-40,,,,,Included,170.00,74.13,70.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-1020-NS,10 OUTLET SINGLE 20 AMP CIRCUIT THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT 'G' POWER,"PD THIN, ONE 20A, 10 OUT CORD",,4.40,5-20P,20 AMP,"10, 5-20R",37.75,1,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-40-OP,"70"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 70H X 3-1/4W SLOT LACER,,24.80,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL,,14.30,LACE-40-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4025-AV 40 RACK SPACES",6PC 70H X 3-1/4W SLOT LACER,,24.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-4025-AV (Vented Front 25% - Standard Rear),ERK-4025-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE, 40 SPACE 70"" RACKING HEIGHT WITH TWO 20 OUTLET THIN POWER STRIPS",,,VFD-40,,,,Included,170.00,74.13,70.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-1020-NS,10 OUTLET SINGLE 20 AMP CIRCUIT THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT 'G' POWER,"PD THIN, ONE 20A, 10 OUT CORD",,4.40,5-20P,20 AMP,"10, 5-20R",37.75,1,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-40-OP,"70"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 70H X 3-1/4W SLOT LACER,,24.80,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL,,14.30,LACE-40-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4025-AV 40 RACK SPACES",6PC 70H X 3-1/4W SLOT LACER,,24.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4025-AV (Vented Front 64% - Standard Rear),ERK-4025-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE, 40 SPACE 70"" RACKING HEIGHT WITH TWO 20 OUTLET THIN POWER STRIPS",,,,LVFD-40,,,Included,170.00,74.13,70.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-1020-NS,10 OUTLET SINGLE 20 AMP CIRCUIT THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT 'G' POWER,"PD THIN, ONE 20A, 10 OUT CORD",,4.40,5-20P,20 AMP,"10, 5-20R",37.75,1,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-40-OP,"70"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 70H X 3-1/4W SLOT LACER,,24.80,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL,,14.30,LACE-40-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4025-AV 40 RACK SPACES",6PC 70H X 3-1/4W SLOT LACER,,24.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4420 (No Front - Standard Rear),ERK-4420,ERK SERIES,"19"" STAND ALONE ENCLOSURE, 44 SPACE, 77"" RACKING HEIGHT",,,,,,,Included,158.00,81.13,77.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,0,0,1
ERK-4420 (Solid Front - Standard Rear),ERK-4420,ERK SERIES,"19"" STAND ALONE ENCLOSURE, 44 SPACE, 77"" RACKING HEIGHT",FD-44,,,,,,Included,158.00,81.13,77.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4420 (Plexiglas Front - Standard Rear),ERK-4420,ERK SERIES,"19"" STAND ALONE ENCLOSURE, 44 SPACE, 77"" RACKING HEIGHT",,PFD-44,,,,,Included,158.00,81.13,77.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-4420 (Vented Front 25% - Standard Rear),ERK-4420,ERK SERIES,"19"" STAND ALONE ENCLOSURE, 44 SPACE, 77"" RACKING HEIGHT",,,VFD-44,,,,Included,158.00,81.13,77.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4420 (Vented Front 64% - Standard Rear),ERK-4420,ERK SERIES,"19"" STAND ALONE ENCLOSURE, 44 SPACE, 77"" RACKING HEIGHT",,,,LVFD-44,,,Included,158.00,81.13,77.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4420 (Plexi Vented Front - Standard Rear),ERK-4420,ERK SERIES,"19"" STAND ALONE ENCLOSURE, 44 SPACE, 77"" RACKING HEIGHT",,,,,PVFD-44,,Included,158.00,81.13,77.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-4425 (No Front - Standard Rear),ERK-4425,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT ",,,,,,,Included,199.00,81.13,77.13,20.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4425-AV 44 RACK SPACES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,0,0,1
ERK-4425 (Solid Front - Standard Rear),ERK-4425,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT ",FD-44,,,,,,Included,199.00,81.13,77.13,20.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4425-AV 44 RACK SPACES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4425 (Plexiglas Front - Standard Rear),ERK-4425,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT ",,PFD-44,,,,,Included,199.00,81.13,77.13,20.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4425-AV 44 RACK SPACES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-4425 (Vented Front 25% - Standard Rear),ERK-4425,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT ",,,VFD-44,,,,Included,199.00,81.13,77.13,20.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4425-AV 44 RACK SPACES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4425 (Vented Front 64% - Standard Rear),ERK-4425,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT ",,,,LVFD-44,,,Included,199.00,81.13,77.13,20.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4425-AV 44 RACK SPACES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4425 (Plexi Vented Front - Standard Rear),ERK-4425,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT ",,,,,PVFD-44,,Included,199.00,81.13,77.13,20.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4425-AV 44 RACK SPACES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-4425-AV (No Front - Standard Rear),ERK-4425-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT WITH ONE 20 OUTLET THIN POWER STRIP",,,,,,,Included,199.00,81.13,77.13,20.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4425-AV 44 RACK SPACES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,0,0,1
ERK-4425-AV (Solid Front - Standard Rear),ERK-4425-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT WITH ONE 20 OUTLET THIN POWER STRIP",INCLUDED,,,,,,Included,199.00,81.13,77.13,20.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4425-AV 44 RACK SPACES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4425-AV (Plexiglas Front - Standard Rear),ERK-4425-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT WITH ONE 20 OUTLET THIN POWER STRIP",,PFD-44,,,,,Included,199.00,81.13,77.13,20.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4425-AV 44 RACK SPACES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-4425-AV (Vented Front 25% - Standard Rear),ERK-4425-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT WITH ONE 20 OUTLET THIN POWER STRIP",,,VFD-44,,,,Included,199.00,81.13,77.13,20.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4425-AV 44 RACK SPACES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4425-AV (Vented Front 64% - Standard Rear),ERK-4425-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT WITH ONE 20 OUTLET THIN POWER STRIP",,,,LVFD-44,,,Included,199.00,81.13,77.13,20.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4425-AV 44 RACK SPACES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4425-AV (Plexi Vented Front - Standard Rear),ERK-4425-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT WITH ONE 20 OUTLET THIN POWER STRIP",,,,,PVFD-44,,Included,199.00,81.13,77.13,20.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4425-AV 44 RACK SPACES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-1820 (No Front - Partial Vented Rear,ERK-1820,ERK SERIES,"19"" STAND ALONE ENCLOSURE 18 SPACE 31.5"" RACKING HEIGHT",,,,,,ERK-VRD-18,,94.00,35.63,31.63,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR18,"11 GAUGE, 10-32 THREADED 18 SPACE ADDITIONAL RAIL KIT, MOUNTING HARDWARE INCLUDED",18SP ERK REAR RAIL OPTION,,6.70,ERK-RR18,18 SPACE (31.50) ERK REAR RAIL KIT,18SP ERK REAR RAIL ,,6.70,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,0,0,1
ERK-1820 (Solid Front - Partial Vented Rear),ERK-1820,ERK SERIES,"19"" STAND ALONE ENCLOSURE 18 SPACE 31.5"" RACKING HEIGHT",FD-18,,,,,ERK-VRD-18,,94.00,35.63,31.63,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR18,"11 GAUGE, 10-32 THREADED 18 SPACE ADDITIONAL RAIL KIT, MOUNTING HARDWARE INCLUDED",18SP ERK REAR RAIL OPTION,,6.70,ERK-RR18,18 SPACE (31.50) ERK REAR RAIL KIT,18SP ERK REAR RAIL ,,6.70,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-1820 (Plexiglas Front - Partial Vented Rear),ERK-1820,ERK SERIES,"19"" STAND ALONE ENCLOSURE 18 SPACE 31.5"" RACKING HEIGHT",,PFD-18,,,,ERK-VRD-18,,94.00,35.63,31.63,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR18,"11 GAUGE, 10-32 THREADED 18 SPACE ADDITIONAL RAIL KIT, MOUNTING HARDWARE INCLUDED",18SP ERK REAR RAIL OPTION,,6.70,ERK-RR18,18 SPACE (31.50) ERK REAR RAIL KIT,18SP ERK REAR RAIL ,,6.70,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,1,0,1
ERK-1820 (Vented Front 25%  - Partial Vented Rear),ERK-1820,ERK SERIES,"19"" STAND ALONE ENCLOSURE 18 SPACE 31.5"" RACKING HEIGHT",,,VFD-18,,,ERK-VRD-18,,94.00,35.63,31.63,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR18,"11 GAUGE, 10-32 THREADED 18 SPACE ADDITIONAL RAIL KIT, MOUNTING HARDWARE INCLUDED",18SP ERK REAR RAIL OPTION,,6.70,ERK-RR18,18 SPACE (31.50) ERK REAR RAIL KIT,18SP ERK REAR RAIL ,,6.70,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-1820 (Vented Front 64%  - Partial Vented Rear),ERK-1820,ERK SERIES,"19"" STAND ALONE ENCLOSURE 18 SPACE 31.5"" RACKING HEIGHT",,,,LVFD-18,,ERK-VRD-18,,94.00,35.63,31.63,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR18,"11 GAUGE, 10-32 THREADED 18 SPACE ADDITIONAL RAIL KIT, MOUNTING HARDWARE INCLUDED",18SP ERK REAR RAIL OPTION,,6.70,ERK-RR18,18 SPACE (31.50) ERK REAR RAIL KIT,18SP ERK REAR RAIL ,,6.70,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-1825 (No Front - Partial Vented Rear),ERK-1825,ERK SERIES,"19"" STAND ALONE ENCLOSURE 18 SPACE 31.5"" RACKING HEIGHT",,,,,,ERK-VRD-18,,104.00,35.63,31.63,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR18,18 SPACE (31.50) ERK REAR RAIL KIT,18SP ERK REAR RAIL ,,6.70,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,0,0,1
ERK-1825 (Solid Front - Partial Vented Rear),ERK-1825,ERK SERIES,"19"" STAND ALONE ENCLOSURE 18 SPACE 31.5"" RACKING HEIGHT",FD-18,,,,,ERK-VRD-18,,104.00,35.63,31.63,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR18,18 SPACE (31.50) ERK REAR RAIL KIT,18SP ERK REAR RAIL ,,6.70,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-1825 (Plexiglas Front - Partial Vented Rear),ERK-1825,ERK SERIES,"19"" STAND ALONE ENCLOSURE 18 SPACE 31.5"" RACKING HEIGHT",,PFD-18,,,,ERK-VRD-18,,104.00,35.63,31.63,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR18,18 SPACE (31.50) ERK REAR RAIL KIT,18SP ERK REAR RAIL ,,6.70,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,1,0,1
ERK-1825 (Vented Front 25% - Partial Vented Rear),ERK-1825,ERK SERIES,"19"" STAND ALONE ENCLOSURE 18 SPACE 31.5"" RACKING HEIGHT",,,VFD-18,,,ERK-VRD-18,,104.00,35.63,31.63,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR18,18 SPACE (31.50) ERK REAR RAIL KIT,18SP ERK REAR RAIL ,,6.70,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-1825 (Vented Front 64% - Partial Vented Rear),ERK-1825,ERK SERIES,"19"" STAND ALONE ENCLOSURE 18 SPACE 31.5"" RACKING HEIGHT",,,,LVFD-18,,ERK-VRD-18,,104.00,35.63,31.63,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR18,18 SPACE (31.50) ERK REAR RAIL KIT,18SP ERK REAR RAIL ,,6.70,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2120 (No Front - Partial Vented Rear),ERK-2120,ERK SERIES,"19"" STAND ALONE ENCLOSURE 21 SPACE 36.75"" RACKING HEIGHT",,,,,,ERK-VRD-21,,100.00,40.88,38.88,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR21,"11 GAUGE, 10-32 THREADED, 21 SPACE ADDITIONAL RAIL KIT, MOUNTING HARDWARE INCLUDED",21SP ERK REAR RAIL OPTION,,7.90,ERK-RR21,21 SPACE (36.75) ERK REAR RAIL KIT,21SP ERK REAR RAIL ,,7.90,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,0,0,1
ERK-2120 (Solid Front - Partial Vented Rear),ERK-2120,ERK SERIES,"19"" STAND ALONE ENCLOSURE 21 SPACE 36.75"" RACKING HEIGHT",FD-21,,,,,ERK-VRD-21,,100.00,40.88,38.88,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR21,"11 GAUGE, 10-32 THREADED, 21 SPACE ADDITIONAL RAIL KIT, MOUNTING HARDWARE INCLUDED",21SP ERK REAR RAIL OPTION,,7.90,ERK-RR21,21 SPACE (36.75) ERK REAR RAIL KIT,21SP ERK REAR RAIL ,,7.90,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2120 (Plexiglas Front - Partial Vented Rear),ERK-2120,ERK SERIES,"19"" STAND ALONE ENCLOSURE 21 SPACE 36.75"" RACKING HEIGHT",,PFD-21,,,,ERK-VRD-21,,100.00,40.88,38.88,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR21,"11 GAUGE, 10-32 THREADED, 21 SPACE ADDITIONAL RAIL KIT, MOUNTING HARDWARE INCLUDED",21SP ERK REAR RAIL OPTION,,7.90,ERK-RR21,21 SPACE (36.75) ERK REAR RAIL KIT,21SP ERK REAR RAIL ,,7.90,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,1,0,1
ERK-2120 (Vented Front 25% - Partial Vented Rear),ERK-2120,ERK SERIES,"19"" STAND ALONE ENCLOSURE 21 SPACE 36.75"" RACKING HEIGHT",,,VFD-21,,,ERK-VRD-21,,100.00,40.88,38.88,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR21,"11 GAUGE, 10-32 THREADED, 21 SPACE ADDITIONAL RAIL KIT, MOUNTING HARDWARE INCLUDED",21SP ERK REAR RAIL OPTION,,7.90,ERK-RR21,21 SPACE (36.75) ERK REAR RAIL KIT,21SP ERK REAR RAIL ,,7.90,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2120 (Vented Front 64% - Partial Vented Rear),ERK-2120,ERK SERIES,"19"" STAND ALONE ENCLOSURE 21 SPACE 36.75"" RACKING HEIGHT",,,,LVFD-21,,ERK-VRD-21,,100.00,40.88,38.88,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR21,"11 GAUGE, 10-32 THREADED, 21 SPACE ADDITIONAL RAIL KIT, MOUNTING HARDWARE INCLUDED",21SP ERK REAR RAIL OPTION,,7.90,ERK-RR21,21 SPACE (36.75) ERK REAR RAIL KIT,21SP ERK REAR RAIL ,,7.90,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2125 (No Front  - Partial Vented Rear),ERK-2125,ERK SERIES,"19"" STAND ALONE ENCLOSURE 21 SPACE 36.75"" RACKING HEIGHT",,,,,,ERK-VRD-21,,118.00,40.88,36.88,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR21,21 SPACE (36.75) ERK REAR RAIL KIT,21SP ERK REAR RAIL ,,7.90,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,0,0,1
ERK-2125 (Solid Front - Partial Vented Rear),ERK-2125,ERK SERIES,"19"" STAND ALONE ENCLOSURE 21 SPACE 36.75"" RACKING HEIGHT",FD-21,,,,,ERK-VRD-21,,118.00,40.88,36.88,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR21,21 SPACE (36.75) ERK REAR RAIL KIT,21SP ERK REAR RAIL ,,7.90,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2125 (Plexiglas Front - Partial Vented Rear,ERK-2125,ERK SERIES,"19"" STAND ALONE ENCLOSURE 21 SPACE 36.75"" RACKING HEIGHT",,PFD-21,,,,ERK-VRD-21,,118.00,40.88,36.88,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR21,21 SPACE (36.75) ERK REAR RAIL KIT,21SP ERK REAR RAIL ,,7.90,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,1,0,1
ERK-2125 (Vented Front 25% - Partial Vented Rear),ERK-2125,ERK SERIES,"19"" STAND ALONE ENCLOSURE 21 SPACE 36.75"" RACKING HEIGHT",,,VFD-21,,,ERK-VRD-21,,118.00,40.88,36.88,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR21,21 SPACE (36.75) ERK REAR RAIL KIT,21SP ERK REAR RAIL ,,7.90,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2125 (Vented Front 64% - Partial Vented Rear),ERK-2125,ERK SERIES,"19"" STAND ALONE ENCLOSURE 21 SPACE 36.75"" RACKING HEIGHT",,,,LVFD-21,,ERK-VRD-21,,118.00,40.88,36.88,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR21,21 SPACE (36.75) ERK REAR RAIL KIT,21SP ERK REAR RAIL ,,7.90,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2720 (No Front - Partial Vented Rear),ERK-2720,ERK SERIES,"19"" STAND ALONE ENCLOSURE 27 SPACE 47.5"" RACKING HEIGHT",,,,,,ERK-VRD-27,,116.00,51.38,47.38,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR27,"11 GAUGE, 10-32 THREADED, 27 SPACE ADDITIONAL RAIL KIT,  MOUNTING HARDWARE INCLUDED",27SP ERK REAR RAIL OPTION,,10.10,ERK-RR27,27 SPACE (47.25) ERK REAR RAIL KIT,27SP ERK REAR RAIL ,,10.10,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,0,0,1
ERK-2720 (Solid Front - Partial Vented Rear),ERK-2720,ERK SERIES,"19"" STAND ALONE ENCLOSURE 27 SPACE 47.5"" RACKING HEIGHT",FD-27,,,,,ERK-VRD-27,,116.00,51.38,47.38,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR27,"11 GAUGE, 10-32 THREADED, 27 SPACE ADDITIONAL RAIL KIT,  MOUNTING HARDWARE INCLUDED",27SP ERK REAR RAIL OPTION,,10.10,ERK-RR27,27 SPACE (47.25) ERK REAR RAIL KIT,27SP ERK REAR RAIL ,,10.10,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2720 (Plexiglas Front - Partial Vented Rear),ERK-2720,ERK SERIES,"19"" STAND ALONE ENCLOSURE 27 SPACE 47.5"" RACKING HEIGHT",,PFD-27,,,,ERK-VRD-27,,116.00,51.38,47.38,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR27,"11 GAUGE, 10-32 THREADED, 27 SPACE ADDITIONAL RAIL KIT,  MOUNTING HARDWARE INCLUDED",27SP ERK REAR RAIL OPTION,,10.10,ERK-RR27,27 SPACE (47.25) ERK REAR RAIL KIT,27SP ERK REAR RAIL ,,10.10,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,1,0,1
ERK-2720 (Vented Front  25% - Partial Vented Rear),ERK-2720,ERK SERIES,"19"" STAND ALONE ENCLOSURE 27 SPACE 47.5"" RACKING HEIGHT",,,VFD-27,,,ERK-VRD-27,,116.00,51.38,47.38,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR27,"11 GAUGE, 10-32 THREADED, 27 SPACE ADDITIONAL RAIL KIT,  MOUNTING HARDWARE INCLUDED",27SP ERK REAR RAIL OPTION,,10.10,ERK-RR27,27 SPACE (47.25) ERK REAR RAIL KIT,27SP ERK REAR RAIL ,,10.10,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2720 (Vented Front 64% - Partial Vented Rear),ERK-2720,ERK SERIES,"19"" STAND ALONE ENCLOSURE 27 SPACE 47.5"" RACKING HEIGHT",,,,LVFD-27,,ERK-VRD-27,,116.00,51.38,47.38,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR27,"11 GAUGE, 10-32 THREADED, 27 SPACE ADDITIONAL RAIL KIT,  MOUNTING HARDWARE INCLUDED",27SP ERK REAR RAIL OPTION,,10.10,ERK-RR27,27 SPACE (47.25) ERK REAR RAIL KIT,27SP ERK REAR RAIL ,,10.10,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2725 (No Front - Partial Vented Rear),ERK-2725,ERK SERIES,"19"" STAND ALONE ENCLOSURE 27 SPACE 47.5"" RACKING HEIGHT",,,,,,ERK-VRD-27,,132.00,51.38,47.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR27,27 SPACE (47.25) ERK REAR RAIL KIT,27SP ERK REAR RAIL ,,10.10,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,1,0,1
ERK-2725 (Solid Front - Partial Vented Rear),ERK-2725,ERK SERIES,"19"" STAND ALONE ENCLOSURE 27 SPACE 47.5"" RACKING HEIGHT",FD-27,,,,,ERK-VRD-27,,132.00,51.38,47.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR27,27 SPACE (47.25) ERK REAR RAIL KIT,27SP ERK REAR RAIL ,,10.10,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2725 (Plexiglas Front - Partial Vented Rear),ERK-2725,ERK SERIES,"19"" STAND ALONE ENCLOSURE 27 SPACE 47.5"" RACKING HEIGHT",,PFD-27,,,,ERK-VRD-27,,132.00,51.38,47.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR27,27 SPACE (47.25) ERK REAR RAIL KIT,27SP ERK REAR RAIL ,,10.10,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,1,0,1
ERK-2725 (Vented Front 25% - Partial Vented Rear),ERK-2725,ERK SERIES,"19"" STAND ALONE ENCLOSURE 27 SPACE 47.5"" RACKING HEIGHT",,,VFD-27,,,ERK-VRD-27,,132.00,51.38,47.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR27,27 SPACE (47.25) ERK REAR RAIL KIT,27SP ERK REAR RAIL ,,10.10,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2725 (Vented Front 64% - Partial Vented Rear),ERK-2725,ERK SERIES,"19"" STAND ALONE ENCLOSURE 27 SPACE 47.5"" RACKING HEIGHT",,,,LVFD-27,,ERK-VRD-27,,132.00,51.38,47.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR27,27 SPACE (47.25) ERK REAR RAIL KIT,27SP ERK REAR RAIL ,,10.10,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-3520 (No Front- Partial Vented Rear),ERK-3520,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT",,,,,,ERK-VRD-35,,136.00,65.38,61.38,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR35,"11 GAUGE, 10-32 THREADED, 35 SPACE ADDITIONAL RAIL KIT MOUNTING HARDWARE INCLUDED",35SP ERK REAR RAIL OPTION,,12.20,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, FITS ANY 35"" SPACE RACKS, BLACK FINISH",4.5 (3) FAN TOP,,0.00,NONE,NONE,NONE,,0.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,0,0,1
ERK-3520 (Solid Front - Partial Vented Rear),ERK-3520,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT",FD-35,,,,,ERK-VRD-35,,136.00,65.38,61.38,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR35,"11 GAUGE, 10-32 THREADED, 35 SPACE ADDITIONAL RAIL KIT MOUNTING HARDWARE INCLUDED",35SP ERK REAR RAIL OPTION,,12.20,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, FITS ANY 35"" SPACE RACKS, BLACK FINISH",4.5 (3) FAN TOP,,0.00,NONE,NONE,NONE,,0.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-3520 (Plexiglas Front  - Partial Vented Rear),ERK-3520,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT",,PFD-35,,,,ERK-VRD-35,,136.00,65.38,61.38,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR35,"11 GAUGE, 10-32 THREADED, 35 SPACE ADDITIONAL RAIL KIT MOUNTING HARDWARE INCLUDED",35SP ERK REAR RAIL OPTION,,12.20,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, FITS ANY 35"" SPACE RACKS, BLACK FINISH",4.5 (3) FAN TOP,,0.00,NONE,NONE,NONE,,0.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-3520 (Vented Front 25% - Partial Vented Rear),ERK-3520,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT",,,VFD-35,,,ERK-VRD-35,,136.00,65.38,61.38,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR35,"11 GAUGE, 10-32 THREADED, 35 SPACE ADDITIONAL RAIL KIT MOUNTING HARDWARE INCLUDED",35SP ERK REAR RAIL OPTION,,12.20,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, FITS ANY 35"" SPACE RACKS, BLACK FINISH",4.5 (3) FAN TOP,,0.00,NONE,NONE,NONE,,0.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-3520 (Vented Front 64% - Partial Vented Rear),ERK-3520,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT",,,,LVFD-35,,ERK-VRD-35,,136.00,65.38,61.38,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR35,"11 GAUGE, 10-32 THREADED, 35 SPACE ADDITIONAL RAIL KIT MOUNTING HARDWARE INCLUDED",35SP ERK REAR RAIL OPTION,,12.20,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, FITS ANY 35"" SPACE RACKS, BLACK FINISH",4.5 (3) FAN TOP,,0.00,NONE,NONE,NONE,,0.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-3525 (No Front - Partial Vented Rear),ERK-3525,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT",,,,,,ERK-VRD-35,,156.00,65.38,61.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,0,0,1
ERK-3525 (Solid Front - Partial Vented Rear),ERK-3525,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT",FD-35,,,,,ERK-VRD-35,,156.00,65.38,61.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-3525 (Plexiglas Front  - Partial Vented Rear),ERK-3525,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT",,PFD-35,,,,ERK-VRD-35,,156.00,65.38,61.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-3525 (Vented Front 25% - Partial Vented Rear),ERK-3525,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT",,,VFD-35,,,ERK-VRD-35,,156.00,65.38,61.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-3525 (Vented Front 64% - Partial Vented Rear),ERK-3525,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT",,,,LVFD-35,,ERK-VRD-35,,156.00,65.38,61.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-3525-AV (No Front - Partial Vented Rear),ERK-3525-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT WITH TWO 10 OUTLET THIN POWER STRIPS",,,,,,ERK-VRD-35,,210.00,63.39,61.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-1020-NS,10 OUTLET SINGLE 20 AMP CIRCUIT THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT 'G' POWER,"PD THIN, 1-20A, 10 OUT, CORD",,4.40,5-20P,20 AMP,"10, 5-20R",37.75,1,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-37-OP,"64.75"" HEIGHT 3 1/4"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 64-3/4H X 3-1/4W SLOT LCER,,23.10,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,LACE-35-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-3525-AV 37 RACK SPACES",6PC 64-3/4H X 3-1/4W SLOT LCER,,23.10,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,0,0,1
ERK-3525-AV (Solid Front - Partial Vented Rear),ERK-3525-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT WITH TWO 10 OUTLET THIN POWER STRIPS",INCLUDED,,,,,ERK-VRD-35,,210.00,63.39,61.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-1020-NS,10 OUTLET SINGLE 20 AMP CIRCUIT THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT 'G' POWER,"PD THIN, 1-20A, 10 OUT, CORD",,4.40,5-20P,20 AMP,"10, 5-20R",37.75,1,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-37-OP,"64.75"" HEIGHT 3 1/4"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 64-3/4H X 3-1/4W SLOT LCER,,23.10,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,LACE-35-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-3525-AV 37 RACK SPACES",6PC 64-3/4H X 3-1/4W SLOT LCER,,23.10,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-3525-AV (Plexiglas Front - Partial Vented Rear),ERK-3525-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT WITH TWO 10 OUTLET THIN POWER STRIPS",,PFD-35,,,,ERK-VRD-35,,210.00,63.39,61.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-1020-NS,10 OUTLET SINGLE 20 AMP CIRCUIT THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT 'G' POWER,"PD THIN, 1-20A, 10 OUT, CORD",,4.40,5-20P,20 AMP,"10, 5-20R",37.75,1,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-37-OP,"64.75"" HEIGHT 3 1/4"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 64-3/4H X 3-1/4W SLOT LCER,,23.10,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,LACE-35-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-3525-AV 37 RACK SPACES",6PC 64-3/4H X 3-1/4W SLOT LCER,,23.10,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-3525-AV (Vented Front 25% - Partial Vented Rear),ERK-3525-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT WITH TWO 10 OUTLET THIN POWER STRIPS",,,VFD-35,,,ERK-VRD-35,,210.00,63.39,61.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-1020-NS,10 OUTLET SINGLE 20 AMP CIRCUIT THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT 'G' POWER,"PD THIN, 1-20A, 10 OUT, CORD",,4.40,5-20P,20 AMP,"10, 5-20R",37.75,1,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-37-OP,"64.75"" HEIGHT 3 1/4"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 64-3/4H X 3-1/4W SLOT LCER,,23.10,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,LACE-35-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-3525-AV 37 RACK SPACES",6PC 64-3/4H X 3-1/4W SLOT LCER,,23.10,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-3525-AV (Vented Front 64% - Partial Vented Rear),ERK-3525-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT WITH TWO 10 OUTLET THIN POWER STRIPS",,,,LVFD-35,,ERK-VRD-35,,210.00,63.39,61.38,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-1020-NS,10 OUTLET SINGLE 20 AMP CIRCUIT THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT 'G' POWER,"PD THIN, 1-20A, 10 OUT, CORD",,4.40,5-20P,20 AMP,"10, 5-20R",37.75,1,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-37-OP,"64.75"" HEIGHT 3 1/4"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 64-3/4H X 3-1/4W SLOT LCER,,23.10,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,LACE-35-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-3525-AV 37 RACK SPACES",6PC 64-3/4H X 3-1/4W SLOT LCER,,23.10,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4020 (No Front - Partial Vented Rear),ERK-4020,ERK SERIES,"19"" STAND ALONE ENCLOSURE 40 SPACE 70"" RACKING HEIGHT",,,,,,ERK-VRD-40,,150.00,74.13,70.13,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR40,"11 GAUGE, 10-32 THREADED, 40 SPACE ADDITIONAL RAIL KIT MOUNTING HARDWARE INCLUDED",40SP ERK REAR RAIL OPTION,,14.30,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL ,,14.30,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, FITS 35+ SPACE RACKS BLACK FINISH",4.5 (3) FAN TOP,,0.00,NONE,NONE,NONE,,0.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,0,0,1
ERK-4020 (Solid Front - Partial Vented Rear),ERK-4020,ERK SERIES,"19"" STAND ALONE ENCLOSURE 40 SPACE 70"" RACKING HEIGHT",FD-40,,,,,ERK-VRD-40,,150.00,74.13,70.13,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR40,"11 GAUGE, 10-32 THREADED, 40 SPACE ADDITIONAL RAIL KIT MOUNTING HARDWARE INCLUDED",40SP ERK REAR RAIL OPTION,,14.30,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL ,,14.30,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, FITS 35+ SPACE RACKS BLACK FINISH",4.5 (3) FAN TOP,,0.00,NONE,NONE,NONE,,0.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4020 (Plexiglas Front - Partial Vented Rear),ERK-4020,ERK SERIES,"19"" STAND ALONE ENCLOSURE 40 SPACE 70"" RACKING HEIGHT",,PFD-40,,,,ERK-VRD-40,,150.00,74.13,70.13,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR40,"11 GAUGE, 10-32 THREADED, 40 SPACE ADDITIONAL RAIL KIT MOUNTING HARDWARE INCLUDED",40SP ERK REAR RAIL OPTION,,14.30,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL ,,14.30,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, FITS 35+ SPACE RACKS BLACK FINISH",4.5 (3) FAN TOP,,0.00,NONE,NONE,NONE,,0.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-4020 (Vented Front 25% - Partial Vented Rear),ERK-4020,ERK SERIES,"19"" STAND ALONE ENCLOSURE 40 SPACE 70"" RACKING HEIGHT",,,VFD-40,,,ERK-VRD-40,,150.00,74.13,70.13,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR40,"11 GAUGE, 10-32 THREADED, 40 SPACE ADDITIONAL RAIL KIT MOUNTING HARDWARE INCLUDED",40SP ERK REAR RAIL OPTION,,14.30,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL ,,14.30,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, FITS 35+ SPACE RACKS BLACK FINISH",4.5 (3) FAN TOP,,0.00,NONE,NONE,NONE,,0.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4020 (Vented Front 64% - Partial Vented Rear),ERK-4020,ERK SERIES,"19"" STAND ALONE ENCLOSURE 40 SPACE 70"" RACKING HEIGHT",,,,LVFD-40,,ERK-VRD-40,,150.00,74.13,70.13,20.00,23.50,15.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,NONE,NONE,NONE,,0.00,ERK-RR40,"11 GAUGE, 10-32 THREADED, 40 SPACE ADDITIONAL RAIL KIT MOUNTING HARDWARE INCLUDED",40SP ERK REAR RAIL OPTION,,14.30,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL ,,14.30,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, FITS 35+ SPACE RACKS BLACK FINISH",4.5 (3) FAN TOP,,0.00,NONE,NONE,NONE,,0.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4025 (No Front - Partial Vented Rear),ERK-4025,ERK SERIES,"19"" STAND ALONE ENCLOSURE 40 SPACE WITH TWO 10 OUTLET THIN POWER STRIPS",,,,,,ERK-VRD-40,,190.00,74.13,70.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL ,,14.30,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,0,0,1
ERK-4025 (Solid Front - Partial Vented Rear),ERK-4025,ERK SERIES,"19"" STAND ALONE ENCLOSURE 40 SPACE WITH TWO 10 OUTLET THIN POWER STRIPS",FD-40,,,,,ERK-VRD-40,,190.00,74.13,70.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL ,,14.30,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4025 (Plexiglas Front - Partial Vented Rear),ERK-4025,ERK SERIES,"19"" STAND ALONE ENCLOSURE 40 SPACE WITH TWO 10 OUTLET THIN POWER STRIPS",,PFD-40,,,,ERK-VRD-40,,190.00,74.13,70.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL ,,14.30,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-4025 (Vented Front 25% - Partial Vented Rear),ERK-4025,ERK SERIES,"19"" STAND ALONE ENCLOSURE 40 SPACE WITH TWO 10 OUTLET THIN POWER STRIPS",,,VFD-40,,,ERK-VRD-40,,190.00,74.13,70.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL ,,14.30,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4025 (Vented Front 64% - Partial Vented Rear),ERK-4025,ERK SERIES,"19"" STAND ALONE ENCLOSURE 40 SPACE WITH TWO 10 OUTLET THIN POWER STRIPS",,,,LVFD-40,,ERK-VRD-40,,190.00,74.13,70.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL ,,14.30,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4025-AV (No Front - Partial Vented Rear),ERK-4025-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE, 40 SPACE 70"" RACKING HEIGHT WITH TWO 20 OUTLET THIN POWER STRIPS",,,,,,ERK-VRD-40,,170.00,74.13,70.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-1020-NS,10 OUTLET SINGLE 20 AMP CIRCUIT THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT 'G' POWER,"PD THIN, ONE 20A, 10 OUT CORD",,4.40,5-20P,20 AMP,"10, 5-20R",37.75,1,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-40-OP,"70"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 70H X 3-1/4W SLOT LACER,,24.80,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL,,14.30,LACE-40-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4025-AV 40 RACK SPACES",6PC 70H X 3-1/4W SLOT LACER,,24.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,0,0,1
ERK-4025-AV (Solid Front - Partial Vented Rear),ERK-4025-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE, 40 SPACE 70"" RACKING HEIGHT WITH TWO 20 OUTLET THIN POWER STRIPS",FD-40,,,,,ERK-VRD-40,,170.00,74.13,70.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-1020-NS,10 OUTLET SINGLE 20 AMP CIRCUIT THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT 'G' POWER,"PD THIN, ONE 20A, 10 OUT CORD",,4.40,5-20P,20 AMP,"10, 5-20R",37.75,1,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-40-OP,"70"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 70H X 3-1/4W SLOT LACER,,24.80,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL,,14.30,LACE-40-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4025-AV 40 RACK SPACES",6PC 70H X 3-1/4W SLOT LACER,,24.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4025-AV (Plexiglas Front - Partial Vented Rear),ERK-4025-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE, 40 SPACE 70"" RACKING HEIGHT WITH TWO 20 OUTLET THIN POWER STRIPS",,PFD-40,,,,ERK-VRD-40,,170.00,74.13,70.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-1020-NS,10 OUTLET SINGLE 20 AMP CIRCUIT THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT 'G' POWER,"PD THIN, ONE 20A, 10 OUT CORD",,4.40,5-20P,20 AMP,"10, 5-20R",37.75,1,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-40-OP,"70"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 70H X 3-1/4W SLOT LACER,,24.80,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL,,14.30,LACE-40-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4025-AV 40 RACK SPACES",6PC 70H X 3-1/4W SLOT LACER,,24.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-4025-AV (Vented Front 25% - Partial Vented Rear),ERK-4025-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE, 40 SPACE 70"" RACKING HEIGHT WITH TWO 20 OUTLET THIN POWER STRIPS",,,VFD-40,,,ERK-VRD-40,,170.00,74.13,70.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-1020-NS,10 OUTLET SINGLE 20 AMP CIRCUIT THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT 'G' POWER,"PD THIN, ONE 20A, 10 OUT CORD",,4.40,5-20P,20 AMP,"10, 5-20R",37.75,1,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-40-OP,"70"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 70H X 3-1/4W SLOT LACER,,24.80,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL,,14.30,LACE-40-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4025-AV 40 RACK SPACES",6PC 70H X 3-1/4W SLOT LACER,,24.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4025-AV (Vented Front 64% - Partial Vented Rear),ERK-4025-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE, 40 SPACE 70"" RACKING HEIGHT WITH TWO 20 OUTLET THIN POWER STRIPS",,,,LVFD-40,,ERK-VRD-40,,170.00,74.13,70.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-1020-NS,10 OUTLET SINGLE 20 AMP CIRCUIT THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT 'G' POWER,"PD THIN, ONE 20A, 10 OUT CORD",,4.40,5-20P,20 AMP,"10, 5-20R",37.75,1,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-40-OP,"70"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 70H X 3-1/4W SLOT LACER,,24.80,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL,,14.30,LACE-40-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4025-AV 40 RACK SPACES",6PC 70H X 3-1/4W SLOT LACER,,24.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4 1/2"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN / TOP W/FC ERK,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4420 (No Front - Partial Vented Rear),ERK-4420,ERK SERIES,"19"" STAND ALONE ENCLOSURE, 44 SPACE, 77"" RACKING HEIGHT",,,,,,ERK-VRD-44,,158.00,81.13,77.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,0,0,1
ERK-4420 (Solid Front - Partial Vented Rear),ERK-4420,ERK SERIES,"19"" STAND ALONE ENCLOSURE, 44 SPACE, 77"" RACKING HEIGHT",FD-44,,,,,ERK-VRD-44,,158.00,81.13,77.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4420 (Plexiglas Front - Partial Vented Rear),ERK-4420,ERK SERIES,"19"" STAND ALONE ENCLOSURE, 44 SPACE, 77"" RACKING HEIGHT",,PFD-44,,,,ERK-VRD-44,,158.00,81.13,77.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-4420 (Vented Front 25% - Partial Vented Rear),ERK-4420,ERK SERIES,"19"" STAND ALONE ENCLOSURE, 44 SPACE, 77"" RACKING HEIGHT",,,VFD-44,,,ERK-VRD-44,,158.00,81.13,77.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4420 (Vented Front 64% - Partial Vented Rear),ERK-4420,ERK SERIES,"19"" STAND ALONE ENCLOSURE, 44 SPACE, 77"" RACKING HEIGHT",,,,LVFD-44,,ERK-VRD-44,,158.00,81.13,77.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4420 (Plexi Vented Front - Partial Vented Rear),ERK-4420,ERK SERIES,"19"" STAND ALONE ENCLOSURE, 44 SPACE, 77"" RACKING HEIGHT",,,,,PVFD-44,ERK-VRD-44,,158.00,81.13,77.13,25.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-25,"COMMERCIAL GRADE CASTER BASE FOR 25"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 25 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-4425 (No Front - Partial Vented Rear),ERK-4425,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT ",,,,,,ERK-VRD-44,,199.00,81.13,77.13,20.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4425-AV 44 RACK SPACES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,0,0,1
ERK-4425 (Solid Front - Partial Vented Rear),ERK-4425,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT ",FD-44,,,,,ERK-VRD-44,,199.00,81.13,77.13,20.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4425-AV 44 RACK SPACES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4425 (Plexiglas Front - Partial Vented Rear),ERK-4425,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT ",,PFD-44,,,,ERK-VRD-44,,199.00,81.13,77.13,20.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4425-AV 44 RACK SPACES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-4425 (Vented Front 25% - Partial Vented Rear),ERK-4425,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT ",,,VFD-44,,,ERK-VRD-44,,199.00,81.13,77.13,20.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4425-AV 44 RACK SPACES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4425 (Vented Front 64% - Partial Vented Rear),ERK-4425,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT ",,,,LVFD-44,,ERK-VRD-44,,199.00,81.13,77.13,20.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4425-AV 44 RACK SPACES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4425 (Plexi Vented Front - Partial Vented Rear),ERK-4425,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT ",,,,,PVFD-44,ERK-VRD-44,,199.00,81.13,77.13,20.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4425-AV 44 RACK SPACES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-4425-AV (No Front - Partial Vented Rear),ERK-4425-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT WITH ONE 20 OUTLET THIN POWER STRIP",,,,,,ERK-VRD-44,,199.00,81.13,77.13,20.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4425-AV 44 RACK SPACES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,0,0,1
ERK-4425-AV (Solid Front - Partial Vented Rear),ERK-4425-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT WITH ONE 20 OUTLET THIN POWER STRIP",INCLUDED,,,,,ERK-VRD-44,,199.00,81.13,77.13,20.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4425-AV 44 RACK SPACES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4425-AV (Plexiglas Front - Partial Vented Rear),ERK-4425-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT WITH ONE 20 OUTLET THIN POWER STRIP",,PFD-44,,,,ERK-VRD-44,,199.00,81.13,77.13,20.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4425-AV 44 RACK SPACES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-4425-AV (Vented Front 25% - Partial Vented Rear),ERK-4425-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT WITH ONE 20 OUTLET THIN POWER STRIP",,,VFD-44,,,ERK-VRD-44,,199.00,81.13,77.13,20.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4425-AV 44 RACK SPACES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4425-AV (Vented Front 64% - Partial Vented Rear),ERK-4425-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT WITH ONE 20 OUTLET THIN POWER STRIP",,,,LVFD-44,,ERK-VRD-44,,199.00,81.13,77.13,20.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4425-AV 44 RACK SPACES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4425-AV (Plexi Vented Front - Partial Vented Rear)),ERK-4425-AV,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT WITH ONE 20 OUTLET THIN POWER STRIP",,,,,PVFD-44,ERK-VRD-44,,199.00,81.13,77.13,20.00,23.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-20,"COMMERCIAL GRADE CASTER BASE FOR 20"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR FOR ERK-4425-AV 44 RACK SPACES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-1828 (No Front - Partial Vented Rear),ERK-1825,ERK SERIES,"19"" STAND ALONE ENCLOSURE 18 SPACE 31.5"" RACKING HEIGHT",,,,,,ERK-VRD-18,,104.00,35.63,31.63,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR18,18 SPACE (31.50) ERK REAR RAIL KIT,18SP ERK REAR RAIL ,,6.70,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,0,0,1
ERK-1828 (Solid Front - Partial Vented Rear),ERK-1828,ERK SERIES,"19"" STAND ALONE ENCLOSURE 18 SPACE 31.5"" RACKING HEIGHT",FD-18,,,,,ERK-VRD-18,,104.00,35.63,31.63,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR18,18 SPACE (31.50) ERK REAR RAIL KIT,18SP ERK REAR RAIL ,,6.70,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-1828 (Plexiglas Front - Partial Vented Rear),ERK-1828,ERK SERIES,"19"" STAND ALONE ENCLOSURE 18 SPACE 31.5"" RACKING HEIGHT",,PFD-18,,,,ERK-VRD-18,,104.00,35.63,31.63,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR18,18 SPACE (31.50) ERK REAR RAIL KIT,18SP ERK REAR RAIL ,,6.70,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,1,0,1
ERK-1828 (Vented Front 25% - Partial Vented Rear),ERK-1825,ERK SERIES,"19"" STAND ALONE ENCLOSURE 18 SPACE 31.5"" RACKING HEIGHT",,,VFD-18,,,ERK-VRD-18,,104.00,35.63,31.63,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR18,18 SPACE (31.50) ERK REAR RAIL KIT,18SP ERK REAR RAIL ,,6.70,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-1828 (Vented Front 64% - Partial Vented Rear),ERK-1825,ERK SERIES,"19"" STAND ALONE ENCLOSURE 18 SPACE 31.5"" RACKING HEIGHT",,,,LVFD-18,,ERK-VRD-18,,104.00,35.63,31.63,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR18,18 SPACE (31.50) ERK REAR RAIL KIT,18SP ERK REAR RAIL ,,6.70,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2128 (Solid Front - Partial Vented Rear),ERK-2128,ERK SERIES,"19"" STAND ALONE ENCLOSURE 21 SPACE 36.75"" RACKING HEIGHT",FD-21,,,,,ERK-VRD-21,,118.00,40.88,36.88,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR21,21 SPACE (36.75) ERK REAR RAIL KIT,21SP ERK REAR RAIL ,,7.90,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2128 (Plexiglas Front - Partial Vented Rear,ERK-2128,ERK SERIES,"19"" STAND ALONE ENCLOSURE 21 SPACE 36.75"" RACKING HEIGHT",,PFD-21,,,,ERK-VRD-21,,118.00,40.88,36.88,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR21,21 SPACE (36.75) ERK REAR RAIL KIT,21SP ERK REAR RAIL ,,7.90,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,1,0,1
ERK-2128 (Vented Front 25% - Partial Vented Rear),ERK-2128,ERK SERIES,"19"" STAND ALONE ENCLOSURE 21 SPACE 36.75"" RACKING HEIGHT",,,VFD-21,,,ERK-VRD-21,,118.00,40.88,36.88,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR21,21 SPACE (36.75) ERK REAR RAIL KIT,21SP ERK REAR RAIL ,,7.90,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2128 (Vented Front 64% - Partial Vented Rear),ERK-2128,ERK SERIES,"19"" STAND ALONE ENCLOSURE 21 SPACE 36.75"" RACKING HEIGHT",,,,LVFD-21,,ERK-VRD-21,,118.00,40.88,36.88,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR21,21 SPACE (36.75) ERK REAR RAIL KIT,21SP ERK REAR RAIL ,,7.90,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2728 (Solid Front - Partial Vented Rear),ERK-2728,ERK SERIES,"19"" STAND ALONE ENCLOSURE 27 SPACE 47.5"" RACKING HEIGHT",FD-27,,,,,ERK-VRD-27,,132.00,51.38,47.38,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR27,27 SPACE (47.25) ERK REAR RAIL KIT,27SP ERK REAR RAIL ,,10.10,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2728 (Plexiglas Front - Partial Vented Rear),ERK-2728,ERK SERIES,"19"" STAND ALONE ENCLOSURE 27 SPACE 47.5"" RACKING HEIGHT",,PFD-27,,,,ERK-VRD-27,,132.00,51.38,47.38,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR27,27 SPACE (47.25) ERK REAR RAIL KIT,27SP ERK REAR RAIL ,,10.10,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,0,1,0,1
ERK-2728 (Vented Front 25% - Partial Vented Rear),ERK-2728,ERK SERIES,"19"" STAND ALONE ENCLOSURE 27 SPACE 47.5"" RACKING HEIGHT",,,VFD-27,,,ERK-VRD-27,,132.00,51.38,47.38,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR27,27 SPACE (47.25) ERK REAR RAIL KIT,27SP ERK REAR RAIL ,,10.10,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-2728 (Vented Front 64% - Partial Vented Rear),ERK-2728,ERK SERIES,"19"" STAND ALONE ENCLOSURE 27 SPACE 47.5"" RACKING HEIGHT",,,,LVFD-27,,ERK-VRD-27,,132.00,51.38,47.38,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR27,27 SPACE (47.25) ERK REAR RAIL KIT,27SP ERK REAR RAIL ,,10.10,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,,0.00,1,1,0,0,1
ERK-3528 (No Front - Standard Rear),ERK-3528,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT",,,,,,,Included,156.00,65.38,61.38,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,0,0,1
ERK-3528 (Solid Front - Standard Rear),ERK-3528,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT",FD-35,,,,,,Included,156.00,65.38,61.38,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-3528 (Plexiglas Front  - Standard Rear),ERK-3528,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT",,PFD-35,,,,,Included,156.00,65.38,61.38,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-3528 (Vented Front 25% - Standard Rear),ERK-3528,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT",,,VFD-35,,,,Included,156.00,65.38,61.38,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-3528 (Vented Front 64% - Standard Rear),ERK-3528,ERK SERIES,"19"" STAND ALONE ENCLOSURE 35 SPACE 61.25"" RACKING HEIGHT",,,,LVFD-35,,,Included,156.00,65.38,61.38,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR35,35 SPACE (61.25) ERK REAR RAIL KIT,35SP ERK REAR RAIL ,,12.20,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4028 (No Front - Partial Vented Rear),ERK-4028,ERK SERIES,"19"" STAND ALONE ENCLOSURE 40 SPACE",,,,,,ERK-VRD-40,,190.00,74.13,70.13,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL ,,14.30,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,0,0,1
ERK-4028 (Solid Front - Partial Vented Rear),ERK-4028,ERK SERIES,"19"" STAND ALONE ENCLOSURE 40 SPACE",FD-40,,,,,ERK-VRD-40,,190.00,74.13,70.13,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL ,,14.30,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4028 (Plexiglas Front - Partial Vented Rear),ERK-4028,ERK SERIES,"19"" STAND ALONE ENCLOSURE 40 SPACE",,PFD-40,,,,ERK-VRD-40,,190.00,74.13,70.13,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL ,,14.30,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-4028 (Vented Front 25% - Partial Vented Rear),ERK-4028,ERK SERIES,"19"" STAND ALONE ENCLOSURE 40 SPACE",,,VFD-40,,,ERK-VRD-40,,190.00,74.13,70.13,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL ,,14.30,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4028 (Vented Front 64% - Partial Vented Rear),ERK-4028,ERK SERIES,"19"" STAND ALONE ENCLOSURE 40 SPACE",,,,LVFD-40,,ERK-VRD-40,,190.00,74.13,70.13,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,NONE,NONE,NONE,,0.00,NONE,NONE,NONE,NONE,NONE,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,NONE,NONE,NONE,,0.00,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL","SKIRTED WHEELBASE, FITS 28 DEEP ERKS, INCLUDES CASTERS",,19.20,ERK-RR40,40 SPACE (70) ERK REAR RAIL KIT,40SP ERK REAR RAIL ,,14.30,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,10 FAN TOP (EXCLUDING FAN)  BLACK FINISH,ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4428 (No Front - Partial Vented Rear),ERK-4428,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT ",,,,,,ERK-VRD-44,,199.00,81.13,77.13,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR ",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,0,0,1
ERK-4428 (Solid Front - Partial Vented Rear),ERK-4428,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT ",FD-44,,,,,ERK-VRD-44,,199.00,81.13,77.13,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4428 (Plexiglas Front - Partial Vented Rear),ERK-4428,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT ",,PFD-44,,,,ERK-VRD-44,,199.00,81.13,77.13,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
ERK-4428 (Vented Front 25% - Partial Vented Rear),ERK-4428,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT ",,,VFD-44,,,ERK-VRD-44,,199.00,81.13,77.13,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR ",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4428 (Vented Front 64% - Partial Vented Rear),ERK-4428,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT ",,,,LVFD-44,,ERK-VRD-44,,199.00,81.13,77.13,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,1,0,0,1
ERK-4428 (Plexi Vented Front - Partial Vented Rear),ERK-4428,ERK SERIES,"19"" STAND ALONE ENCLOSURE 44 SPACE 77"" RACKING HEIGHT ",,,,,PVFD-44,ERK-VRD-44,,199.00,81.13,77.13,28.00,26.50,20.25,UL,RoHS GREENGUARD IAQ for Children and Schools,SECTION 27 11 16 Equipment Enclosures,23-37 11 15 Communication Racks,Racks and Rackmount Systems,www.middleatlantic.com,http://www.middleatlantic.com/enclosure/sa/erksa.htm,UBC IBC CBC ASCE and NFPA Zone 4 and Use Group III,PDT-2020-NS,20 OUTLET SINGLE 20A CIRCUIT WITH CURRENT METER THIN POWER STRIP WITH 9' CORD FITS RACKS THAT ACCEPT  'T'  POWER,"PD THIN ONE 20A, 20 OUT, MTR CORD",,6.50,5-20P,20 AMP,"20, 5-20R",72.78,2,CBS-ERK-28,"COMMERCIAL GRADE CASTER BASE FOR 28"" DEPTH MODEL",CASTER BASE ,,17.50,LACE-44-OP,"77"" HEIGHT 3.25"" WIDTH CABLE LACER STRIP WITH CABLE TIE POSTS, 6 PIECES",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-RR44,44 SPACE (77) ERK REAR RAIL KIT,44SP ERK REAR RAIL ,,15.50,LACE-44-OP,"3.25"" WIDTH VERTICAL LACER BAR",6PC 77H X 3-1/4W SLOT LACER,,26.10,ERK-4FT,"4.5 FAN TOP (EXCLUDING FANS) FITS UP TO 3 FANS, BLACK FINISH",ERK FAN TOP FITS 3PCS UPTO 4 FANS,,5.80,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-4QFT-FC,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 QUIET FANS AND PROPORTIONAL SPEED FAN CONTROL, BLACK FINISH",4.5 (3) FAN TOP,,13.00,ERK-4FT-285CFM,"INTEGRATED 4.5"" FAN TOP, INCLUDES 3 FANS, 285 CFM BLACK FINISH","4"" (1) FANTOP 285CFM BLACK FINISH",,11.00,ERK-6FT,"6 FAN TOP WITHOUT FANS, FITS UP TO 2 FANS, BLACK FINISH",ERK FANTOP FITS 2 FANS,,5.80,ERK-6FT-440CFM,"INTEGRATED 6"" FAN TOP, INCLUDES 2 FANS, 285 CFM, FITS ANY WMRK, ERK-KD, ERK (35+ SPACE ONLY) OR SCRK (44 SPACE ONLY), BLACK FINISH","6"" (1) FANTOP 440CFM, ERK",,10.30,ERK-10FT,"10 FAN TOP (EXCLUDING FAN) FOR ANY WMRK, ERK-KD, SCRK (44 SPACE ONLY) OR ERK (35+ SPACE ONLY) SERIES RACK, BLACK FINISH",ERK FAN TOP FITS 1PC.10FA,,4.70,ERK-10FT-FC,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN AND PROPORTIONAL SPEED FAN CONTROL BLACK FINISH",10 (1) FAN / TOP W/FC ERK,,13.00,ERK-10FT-550CFM,"INTEGRATED 10"" FAN TOP, INCLUDES 1 FAN, 665 CFM,  BLACK FINISH","10"" (1) FANTOP 665CFM, ERK",,8.00,1,0,1,0,1
